NuttX TODO List (Last updated January 30, 2013)
^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

This file summarizes known NuttX bugs, limitations, inconsistencies with 
standards, things that could be improved, and ideas for enhancements.

nuttx/

 (11)  Task/Scheduler (sched/)
  (2)  Memory Managment (mm/)
  (3)  Signals (sched/, arch/)
  (2)  pthreads (sched/)
  (2)  C++ Support
  (6)  Binary loaders (binfmt/)
 (16)  Network (net/, drivers/net)
  (4)  USB (drivers/usbdev, drivers/usbhost)
 (11)  Libraries (libc/, )
  (9)  File system/Generic drivers (fs/, drivers/)
  (5)  Graphics subystem (graphics/)
  (1)  Pascal add-on (pcode/)
  (1)  Documentation (Documentation/)
  (7)  Build system / Toolchains
  (5)  Linux/Cywgin simulation (arch/sim)
  (5)  ARM (arch/arm/)
  (1)  ARM/C5471 (arch/arm/src/c5471/)
  (3)  ARM/DM320 (arch/arm/src/dm320/)
  (2)  ARM/i.MX (arch/arm/src/imx/)
  (3)  ARM/LPC17xx (arch/arm/src/lpc17xx/)
  (7)  ARM/LPC214x (arch/arm/src/lpc214x/)
  (2)  ARM/LPC313x (arch/arm/src/lpc313x/)
  (0)  ARM/LPC43x (arch/arm/src/lpc43xx/)
  (3)  ARM/STR71x (arch/arm/src/str71x/)
  (3)  ARM/LM3S6918 (arch/arm/src/lm/)
  (5)  ARM/STM32 (arch/arm/src/stm32/)
  (3)  AVR (arch/avr)
  (0)  Intel x86 (arch/x86)
  (5)  8051 / MCS51 (arch/8051/)
  (3)  MIPS/PIC32 (arch/mips)
  (1)  Hitachi/Renesas SH-1 (arch/sh/src/sh1)
  (4)  Renesas M16C/26 (arch/sh/src/m16c)
 (11)  z80/z8/ez80/z180 (arch/z80/)
  (9)  z16 (arch/z16/)
  (1)  mc68hc1x (arch/hc)

apps/

  (5)  Network Utilities (apps/netutils/)
  (5)  NuttShell (NSH) (apps/nshlib)
  (1)  System libraries apps/system (apps/system)
  (5)  Other Applications & Tests (apps/examples/)

o Task/Scheduler (sched/)
  ^^^^^^^^^^^^^^^^^^^^^^^

  Title:       CHILD PTHREAD TERMINATION
  Description: When a tasks exits, shouldn't all of its child pthreads also be
               terminated?
  Status:      Closed.  No, this behavior will not be implemented.
  Priority:    Medium, required for good emulation of process/pthread model.

  Title:       TICKLESS OS
  Description: On a side note, I have thought about a tick-less timer for the OS
               for a long time.  Basically we could replace the periodic system
               timer interrupt with a one-shot interval timer programmed for the
               next interesting event time.  That is one way to both reduce the
               timer interrupt overhead and also to increase the accuracy of
               delays.

               Current timer processing is in sched/sched_processtimer.c:

               1) Calls clock_timer() which just increments a counter (the system
                  timer -- basically "up-time"). This is only used when code asks
                  for the current time.  In a tickless OS, some substitute answer
                  for the question "What time is it?" would need to be developed.
                  You could use an RTC? Or maybe logic that gets the time until the
                  next interval expiration and computes the current time. The
                  solution is not too difficult, but depends on a hardware solution.

               2) Calls wd_timer() which handles the link list of ordered events:
                  Each timer event is saved with the delta time to the next event
                  in the list. So an interval timer would be perfect to implement this.

               3) sched_process_timeslice(). Then there is round-robin time-slicing.

               The primary advantage of a tickless OS is that is would allow for
               reduce power consumptions.  That is because timer interrupts will
               usually awaken CPUs from reduced power consumption states.
  Status:      Open.  There will probably be no tickless OS implementation unless
               someone gets motivated and drives the change.
  Priority:    Low

  Title:       pause() NON-COMPLIANCE
  Description: In the POSIX description of this function is the pause() function
               will suspend the calling thread until delivery of a signal whose
               action is either to execute a signal-catching function or to
               terminate the process.  The current implementation only waits for
               any non-blocked signal to be received.  It should only wake up if
               the signal is delivered to a handler.
  Status:      Open.
  Priority:    Medium Low.

  Title:       ON-DEMAND PAGE INCOMPLETE
  Description: On-demand paging has recently been incorporated into the RTOS.
               The design of this feature is described here:
               http://www.nuttx.org/NuttXDemandPaging.html.
               As of this writing, the basic feature implementation is
               complete and much of the logic has been verified.  The test
               harness for the feature exists only for the NXP LPC3131 (see
               configs/ea3131/pgnsh and locked directories).  There are
               some limitations of this testing so I still cannot say that
               the feature is fully functional.
  Status:      Open.  This has been put on the shelf for some time.
  Priority:    Medium-Low

  Title:       GET_ENVIRON_PTR()
  Description: get_environ_ptr() (sched/sched_getenvironptr.c) is not implemented.
               The representation of the the environment strings selected for
               NutX is not compatible with the operation.  Some significant
               re-design would be required to implement this funcion and that
               effort is thought to be not worth the result.
  Status:      Open.  No change is planned.
  Priority:    Low -- There is no plan to implement this.

  Title:       TIMER_GETOVERRUN()
  Description: timer_getoverrun() (sched/timer_getoverrun.c) is not implemented.
  Status:      Open
  Priority:    Low -- There is no plan to implement this.

  Title:       USER-SPACE WORK QUEUES
  Description: There has been some use of work queues that has crept into some
               user code.  I am thinking of NxWidgets::CNxTimer.  That timer
               logic was originally implemented (correctly) using POSIX timers,
               but was re-implemented using timed work.

               The issue is that NxWidgets::CNxTimer is a user-space application
               but the work queues are an OS internal feature.  This will be a
               problem for KERNEL builds.  Hooks and definitions have been added
               in include/nuttx/wqueue.h to support a user-space work queue, but
               the corresponding logic has not been implemented.

               The work queue logic will need to be moved from sched/ to libc/wqueue/
  Status:      Open.  No work will probably be done until a functional KERNEL build
               that includes NxWisges::CNxTimer is needed.
  Priority:    Medium Low for now

  Title:       INCOMPATIBILITES WITH execv() AND execl()
  Description: Simplified 'execl()' and 'execv()' functions are provided by
               NuttX.  NuttX does not support processes and hence the concept
               of overlaying a tasks process image with a new process image
               does not make any sense.  In NuttX, these functions are
               wrapper functions that:

               1. Call the non-standard binfmt function 'exec', and then
               2. exit(0).

               As a result, the current implementations of 'execl()' and
               'execv()' suffer from some incompatibilities, the most
               serious of these is that the exec'ed task will not have
               the same task ID as the vfork'ed function.  So the parent
               function cannot know the ID of the exec'ed task.
  Status:      Open
  Priority:    Medium Low for now

  Title:       ISSUES WITH atexit() AND on_exit()
  Description: These functions execute with the following bad properties:
  
               1. They run with interrupts disabled,
               2. They run in supervisor mode (if applicable), and
               3. They do not obey any setup of PIC or address
                  environments. Do they need to?

               The fix for all of these issues it to have the callbacks
               run on the caller's thread (as with signal handlers).
  Status:      Open
  Priority:    Medium Low.  This is an important change to some less
               important interfaces.  For the average user, these
               functions are just fine the way they are.

  Title:       execv() AND vfork()
  Description: There is a problem when vfork() calls execv() (or execl()) to
               start a new appliction:  When the parent thread calls vfork()
               it receives and gets the pid of the vforked task, and *not*
               the pid of the desired execv'ed application.

               The same tasking arrangement is used by the standard function
               posix_spawn().  However, posix_spawn uses the non-standard, internal
               NuttX interface task_reparent() to replace the childs parent task
               with the caller of posix_spawn().  That cannot be done with vfork()
               because we don't know what vfor() is going to do.

               Any solution to this is either very difficult or impossible with
               an MMU.
  Status:      Open
  Priority:    Low (it might as well be low since it isn't going to be fixed).

  Title:       errno IS NOT SHARED AMONG THREADS
  Description: In NuttX, the errno value is unique for each thread.  But for
               bug-for-bug compatibility, the same errno should be shared by
               the task and each thread that it creates.  It is *very* easy
               to make this change:  Just move the pterrno field from
               _TCB to struct task_group_s.   However, I am still not sure
               if this should be done or not.
  Status:      Open
  Priority:    Low

o Memory Managment (mm/)
  ^^^^^^^^^^^^^^^^^^^^^^

  Title:       FREE MEMORY ON TASK EXIT
  Description: Add an option to free all memory allocated by a task when the
               task exits. This is probably not be worth the overhead for a
               deeply embedded system.

               There would be complexities with this implementation as well
               because often one task allocates memory and then passes the
               memory to another:  The task that "owns" the memory may not
               be the same as the task that allocated the memory.

               Update.  From the NuttX forum:
               ...there is a good reason why task A should never delete task B.
               That is because you will strand memory resources. Another feature
               lacking in most flat address space RTOSs is automatic memory
               clean-up when a task exits.

               That behavior just comes for free in a process-based OS like Linux:
               Each process has its own heap and when you tear down the process
               environment, you naturally destroy the heap too.

               But RTOSs have only a single, shared heap. I have spent some time
               thinking about how you could clean up memory required by a task
               when a task exits. It is not so simple. It is not as simple as
               just keeping memory allocated by a thread in a list then freeing
               the list of allocations when the task exists.

               It is not that simple because you don't know how the memory is
               being used. For example, if task A allocates memory that is used
               by task B, then when task A exits, you would not want to free that
               memory needed by task B. In a process-based system, you would
               have to explicitly map shared memory (with reference counting) in
               order to share memory. So the life of shared memory in that
               environment is easily managed.

               I have thought that the way that this could be solved in NuttX
               would be: (1) add links and reference counts to all memory allocated
               by a thread. This would increase the memory allocation overhead!
               (2) Keep the list head in the TCB, and (3) extend mmap() and munmap()
               to include the shared memory operations (which would only manage
               the reference counting and the life of the allocation).

               Then what about pthreads? Memory should not be freed until the last
               pthread in the group exists. That could be done with an additional
               reference count on the whole allocated memory list (just as streams
               and file descriptors are now shared and persist until the last
               pthread exits).

               I think that would work but to me is very unattractive and
               inconsistent with the NuttX "small footprint" objective. ...

               Other issues:
               - Memory free time would go up because you would have to remove
                 the memory from that list in free().
               - There are special cases inside the RTOS itself.  For example,
                 if task A creates task B, then initial memory allocations for
                 task B are created by task A.  Some special allocators would
                 be required to keep this memory on the correct list (or on
                 no list at all).

  Status:      Open.  No changes are planned.
  Priority:    Medium/Low, a good feature to prevent memory leaks but would
               have negative impact on memory usage and code size.

  Title:       CONTAINER ALLOCATOR
  Description: There are several places where the logic requires allocation of
               a tiny structure that just contains pointers to other things or
               small amounts of data that needs to be bundled together.  There
               are examples net/net_poll.c and numerous other places.

               I am wondering if it would not be good create a pool of generic
               containers (say void *[4]).  There re-use these when we need
               small containers.  The code in sched/task_childstatus.c might
               be generalized for this purpose.
  Status:      Open
  Priority:    Very low (I am not even sure that this is a good idea yet).

o Signals (sched/, arch/)
  ^^^^^^^^^^^^^^^^^^^^^^^

  Title:       STANDARD SIGNALS
  Description: 'Standard' signals and signal actions are not supported.
               (e.g., SIGINT, SIGSEGV, etc).

               Update:  SIG_CHLD is support if configured.
  Status:      Open.  No changes are planned.
  Priority:    Low, required by standards but not so critical for an
               embedded system.

  Title:       SIGEV_THREAD
  Description: sig_notify() logic does not support SIGEV_THREAD; structure
               struct sigevent does not provide required members sigev_notify_function
               or sigev_notify_attributes.
  Status:      Low, there are alternative designs.  However, these features
               are required by the POSIX standard.
  Priority:    Low for now

  Title:       SIGNAL NUMBERING
  Description: In signal.h, the range of valid signals is listed as 0-31.  However,
               in many interfaces, 0 is not a valid signal number.  The valid
               signal number should be 1-32.  The signal set operations would need
               to map bits appropriately.
  Status:      Open
  Priority:    Low. Even if there are only 31 usable signals, that is still a lot.

o pthreads (sched/)
  ^^^^^^^^^^^^^^^^^

  Title:       CANCELLATION POINTS
  Description: pthread_cancel():  Should implement cancellation points and
               pthread_testcancel()
  Status:      Open.  No changes are planned.
  Priority:    Low, probably not that useful

  Title:       PTHREAD_PRIO_PROTECT
  Description: Extended pthread_mutexattr_setprotocol() suport PTHREAD_PRIO_PROTECT:
               "When a thread owns one or more mutexes initialized with the
               PTHREAD_PRIO_PROTECT protocol, it shall execute at the higher of its
               priority  or  the  highest  of the priority ceilings of all the mutexes
               owned by this thread and initialized with this attribute, regardless of
               whether other threads are blocked on any of these mutexes or not.

               "While  a  thread is holding a mutex which has been initialized with
               the PTHREAD_PRIO_INHERIT or PTHREAD_PRIO_PROTECT protocol attributes,
               it shall not be subject to being moved to the tail of the scheduling queue
               at its priority in the event that its original priority is changed,
               such as by a call to sched_setparam(). Likewise, when a thread unlocks
               a mutex that has been initialized with the PTHREAD_PRIO_INHERIT or
               PTHREAD_PRIO_PROTECT protocol attributes, it shall not be subject to
               being moved to the tail of the scheduling queue at its priority in  the
               event that its original priority is changed."
  Status:      Open.  No changes planned.
  Priority:    Low -- about zero, probably not that useful. Priority inheritance is
               already supported and is a much better solution.  And it turns out
               that priority protection is just about as complex as priority inheritance.
               Exerpted from my post in a Linked-In discussion:

               "I started to implement this HLS/"PCP" semaphore in an RTOS that I
               work with (http://www.nuttx.org) and I discovered after doing the
               analysis and basic code framework that a complete solution for the
               case of a counting semaphore is still quite complex -- essentially
               as complex as is priority inheritance.

               "For example, suppose that a thread takes 3 different HLS semaphores
               A, B, and C. Suppose that they are prioritized in that order with
               A the lowest and C the highest. Suppose the thread takes 5 counts
               from A, 3 counts from B, and 2 counts from C. What priority should
               it run at? It would have to run at the priority of the highest
               priority semaphore C. This means that the RTOS must maintain
               internal information of the priority of every semaphore held by
               the thread.

               "Now suppose it releases one count on semaphore B. How does the
               RTOS know that it still holds 2 counts on B? With some complex
               internal data structure. The RTOS would have to maintain internal
               information about how many counts from each semaphore are held
               by each thread.

               "How does the RTOS know that it should not decrement the priority
               from the priority of C? Again, only with internal complexity. It
               would have to know the priority of every semaphore held by
               every thread.

               "Providing the HLS capability on a simple phread mutex would not
               be such quite such a complex job if you allow only one mutex per
               thread. However, the more general case seems almost as complex
               as priority inheritance. I decided that the implementation does
               not have value to me. I only wanted it for its reduced
               complexity; in all other ways I believe that it is the inferior
               solution. So I discarded a few hours of programming. Not a
               big loss from the experience I gained."

o C++ Support
  ^^^^^^^^^^^

  Title:       USE OF SIZE_T IN NEW OPERATOR
  Description: The argument of the 'new' operators should take a type of
               size_t (see libxx/libxx_new.cxx and libxx/libxx_newa.cxx).  But
               size_t has an unknown underlying.  In the nuttx sys/types.h
               header file, size_t is typed as uint32_t (which is determined by
               architecture-specific logic).  But the C++ compiler may believe
               that size_t is of a different type resulting in compilation errors
               in the operator.  Using the underlying integer type Instead of
               size_t seems to resolve the compilation issues.
  Status:      Kind of open.  There is a workaround.  Setting CONFIG_CXX_NEWLONG=y
               will define the operators with argument of type unsigned long;
               Setting CONFIG_CXX_NEWLONG=n will define the operators with argument
               of type unsigned int.  But this is pretty ugly!  A better solution
               would be to get ahold of the compilers definition of size_t.
  Priority:    Low.

  Title:       STATIC CONSTRUCTORS
  Description: Need to call static constructors
               Update:  Static constructors are implemented for the STM32 F4 and
               this will provide the model for all solutions.  Basically, if
               CONFIG_HAVE_CXXINITIALIZE=y is defined in the configuration, then
               board-specific code must provide the interface up_cxxinitialize().
               up_cxxinitialize() is called from user_start() to initialize
               all static class instances.  This TODO item probably has to stay
               open because this solution is only available on STM32 F4.
  Status:      Open
  Priority:    Low, depends on toolchain.  Call to gcc's built-in static
               constructor logic will probably have to be performed by
               user logic in user_start().

o Binary loaders (binfmt/)
  ^^^^^^^^^^^^^^^^^^^^^^^^

  Title:       NXFLAT TESTS
  Description: Not all of the NXFLAT test under apps/examples/nxflat are working.
               Most simply do not compile yet.  tests/mutex runs okay but
               outputs garbage on completion.

               Update: 13-27-1, tests/mutex crashed with a memory corruption
               problem the last time that I ran it.
  Status:      Open
  Priority:    High

  Title:       ARM UP_GETPICBASE()
  Description: The ARM up_getpicbase() does not seem to work.  This means
               the some features like wdog's might not work in NXFLAT modules.
  Status:      Open
  Priority:    Medium-High

  Title:       READ-ONLY DATA IN RAM
  Description: At present, all .rodata must be put into RAM.  There is a 
               tentative design change that might allow .rodata to be placed
               in FLASH (see Documentation/NuttXNxFlat.html).
  Status:      Open
  Priority:    Medium

  Title:       GOT-RELATIVE FUNCTION POINTERS
  Description: If the function pointer to a statically defined function is
               taken, then GCC generates a relocation that cannot be handled
               by NXFLAT.  There is a solution described in Documentataion/NuttXNxFlat.html,
               by that would require a compiler change (which we want to avoid).
               The simple workaround is to make such functions global in scope.
  Status:      Open
  Priority:    Low (probably will not fix)

  Title:       USE A HASH INSTEAD OF A STRING IN SYMBOL TABLES
  Description: In the NXFLAT symbol tables... Using a 32-bit hash value instead
               of a string to identify a symbol should result in a smaller footprint.
  Status:      Open
  Priority:    Low

  Title:       WINDOWS-BASED TOOLCHAIN BUILD
  Description: Windows build issue.  Some of the configurations that use NXFLAT have
               the linker script specified like this:

               NXFLATLDFLAGS2 = $(NXFLATLDFLAGS1) -T$(TOPDIR)/binfmt/libnxflat/gnu-nxflat-gotoff.ld -no-check-sections

               That will not work for windows-based tools because they require Windows
               style paths.  The solution is to do something like this:

               if ($(WINTOOL)y)
                 NXFLATLDSCRIPT=${cygpath -w $(TOPDIR)/binfmt/libnxflat/gnu-nxflat-gotoff.ld}
               else
                 NXFLATLDSCRIPT=$(TOPDIR)/binfmt/libnxflat/gnu-nxflat-gotoff.ld
               endif
               
               Then use
               
               NXFLATLDFLAGS2 = $(NXFLATLDFLAGS1) -T"$(NXFLATLDSCRIPT)" -no-check-sections

  Status:      Open
  Priority:    There are too many references like the above.  They will have
               to get fixed as needed for Windows native tool builds.

  Title:       TOOLCHAIN COMPATIBILITY PROBLEM
  Descripton:  The older 4.3.3 compiler generates GOTOFF relocations to the constant
               strings, like:

               .L3:
                  .word   .LC0(GOTOFF)
                  .word   .LC1(GOTOFF)
                  .word   .LC2(GOTOFF)
                  .word   .LC3(GOTOFF)
                  .word   .LC4(GOTOFF)

               Where .LC0, LC1, LC2, LC3, and .LC4 are the labels correponding to strings in
               the .rodata.str1.1 section.  One consequence of this is that .rodata must reside
               in D-Space since it will addressed relative to the GOT (see the section entitled
               "Read-Only Data in RAM" at
               http://nuttx.org/Documentation/NuttXNxFlat.html#limitations).

               The newer 4.6.3compiler generated PC relative relocations to the strings:

               .L2:
                  .word   .LC0-(.LPIC0+4)
                  .word   .LC1-(.LPIC1+4)
                  .word   .LC2-(.LPIC2+4)
                  .word   .LC3-(.LPIC4+4)
                  .word   .LC4-(.LPIC5+4)

               This is good and bad.  This is good because it means that .rodata.str1.1 can now
               reside in FLASH with .text and can be accessed using PC-relative addressing. 
               That can be accomplished by simply moving the .rodata from the .data section to
               the .text section in the linker script.  (The NXFLAT linker script is located at
               nuttx/binfmt/libnxflat/gnu-nxflat.ld).

               This is bad because a lot of stuff may get broken an a lot of test will need to
               be done.  One question that I have is does this apply to all kinds of .rodata? 
               Or just to .rodata.str1.1?
  
  Status:      Open.  Many of the required changes are in place but, unfortunately, not enough
               go be fully functional.  I think all of the I-Space-to-I-Space fixes are in place.
               However, the generated code also includes PC-relative references to .bss which
               just cannot be done.
  Priority:    Medium.  The workaround for now is to use the older, 4.3.3 OABI compiler.

o Network (net/, drivers/net)
  ^^^^^^^^^^^^^^^^^^^^^^^^^^^

  Title:       SOCK_RAW/SOCK_PACKET
  Description: Should implement SOCK_RAW, SOCK_PACKET
  Status:      Open.  No changes are planned.
  Priority:    Low

  Title:       MULTIPLE NETWORK INTERFACE SUPPORT
  Description: uIP polling issues / Multiple network interface support:

               (1) Current logic will not support multiple ethernet drivers.
                  Each driver should poll on TCP connections connect on the
                  network supported by the driver; UDP polling should respond
                  with TX data only if the UDP packet is intended for the
                  the network supported by the driver.

               (2) If there were multiple drivers, polling would occur at
                  double the rate.  Fix by using bound IP address in TCP
                  connection (lipaddr) and verifying that it is in the subnet
                  served by the driver.

  Status:      Open.  Nothing will probably be done until I have a platform
               with two network interfaces that I need to support.
  Priority:    Medium, The feature is not important, but it is important
               for NuttX to resolve the architectural issues.

  Title:       SENDTO() AND MULTIPLE NETWORK INTERFACE SUPPORT
  Description: sendto() and multiple network interface support:
               When polled, would have to assure that the destination IP
               is on the subnet served by the polling driver.
  Status:      Open.  This is really part of the above issue.
  Priority:    Medium, The feature is not important, but it is important
               for NuttX to resolve the architectural issues.

  Title:       IPv6
  Description: IPv6 support is incomplete.  Adam Dunkels has recently announced
               IPv6 support for uIP (currently only as part of Contiki).  Those
               changes need to be ported to NuttX.
  Status:      Open.  No work will probably be done until there is a specific
               requirement for IPv6.
  Priority:    Medium

  Title:       LISTENING FOR UDP BROADCASTS
  Description: Incoming UDP broadcast should only be accepted if listening on
               INADDR_ANY(?)
  Status:      Open
  Priority:    Low

  Title:       READ-AHEAD THROTTLING
  Description: Read-ahead buffers capture incoming TCP data when no user
               thread is recv-ing the data.  Should add some driver call to
               support throttling; when there is no listener for new data, the
               driver should be throttled.  Perhaps the driver should disable
               RX interrupts when throttled and re-anable on each poll time.
               recvfrom would, of course, have to un-throttle.
  Status:      Open.  This is just a thought experiment.  No changes are planned.
  Priority:    Medium

  Title:       STANDARDIZE ETHERNET DRIVER STATISTICS
  Description: Need to standardize collection of statistics from network
               drivers.  apps/nshlib ifconfig command should present
               statistics.
  Status:      Open
  Priority:    Low

  Title:       CONCURRENT TCP SEND OPERATIONS
  Description: At present, there cannot be two concurrent active TCP send
               operations in progress using the same socket.  This is because
               the uIP ACK logic will support only one transfer at a time.  The
               solution is simple: A mutex will be needed to make sure that each 
               send that is started is able to be the exclusive sender until all of
               the data to be sent has been ACKed.
  Status:      Open.  There is some temporary logic to apps/nshlib that does
               this same fix and that temporary logic should be removed when
               send() is fixed.
  Priority:    Medium-Low.  This is an important issue for applications that
               send on the same TCP socket from multiple threads.

  Title:       UDP READ-AHEAD?
  Description: TCP supports read-ahead buffering to handle the receipt of
               TCP/IP packets when there is no read() in place.  Should such
               capability be useful for UDP?  PRO: Would reduce packet loss
               and enable support for poll()/select().  CON: UDP is inherently
               lossy so why waste memory footprint?
  Status:      Open
  Priority:    Medium

  Title:       NO POLL/SELECT ON UDP SOCKETS
  Description: poll()/select() is not implemented for UDP sockets because they do
               do not support read-ahead buffering.  Therefore, there is never
               a case where you can read from a UDP socket without blocking.
  Status:      Open, depends on UDP read-ahead support
  Priority:    Medium

  Title:       POLL/SELECT ON TCP SOCKETS NEEDS READ-AHEAD
  Description: poll()/select() only works for availability of buffered TCP
               read data (when read-ahead is enabled).  The way writing is
               handled in uIP, all sockets must wait when send and cannot
               be notifiied when they can send without waiting.
  Status:      Open, probably will not be fixed.
  Priority:    Medium... this does effect porting of applications that expect
               different behavior from poll()/select()

  Title:       SOCKETS DO NOT ALWAYS SUPPORT O_NONBLOCK
  Description: sockets do not support all modes for O_NONBLOCK. Sockets
               support only (1) TCP/IP non-blocking read operations when read-ahead
               buffering is enabled, and (2) TCP/IP accept() operations when TCP/IP
               connection backlog is enabled.
  Status:      Open
  Priority:    Low.

  Title:       UNFINISHED CRYSTALLAN CS89X0 DRIVER
  Description: I started coding a CrystalLan CS89x0 driver (drivers/net/cs89x0.c),
               but never finished it.
  Status:      Open
  Priority:    Low unless you need it.

  Title:       UNTESTED IGMPv2
  Description: Support for client-side IGMPv2 multicast has been added but not yet
               tested (because I don't have a proper environment for multicast testing).
               There are most likely errors that need to be fixed at least in the
               receipt of multicast packets.

               In addition, an ethernet driver that needs to work with the IGMP logic
               will have to include additional support for multicast MAC address tables.
  Status:      Open
  Priority:    Low unless you need it.

  Title:       INTERFACES TO LEAVE/JOIN IGMP MULTICAST GROUP
  Description: The interfaces used to leave/join IGMP multicast groups is non-standard.
               RFC3678 (IGMPv3) suggests ioctl() commands to do this (SIOCSIPMSFILTER) but
               also status that those APIs are historic.  NuttX implements these ioctl
               commands, but is non-standard because:  (1) It does not support IGMPv3, and
               (2) it looks up drivers by their device name (eg., "eth0") vs IP address.

               Linux uses setsockopt() to control multicast group membership using the
               IP_ADD_MEMBERSHIP and IP_DROP_MEMBERSHIP options.  It also looks up drivers
               using IP addresses (It would require additional logic in NuttX to look up
               drivers by IP address).  See http://tldp.org/HOWTO/Multicast-HOWTO-6.html
  Status:      Open
  Priority:    Medium.  All standards compatibility is important to NuttX.  However, most
               the mechanism for leaving and joining groups is hidden behind a wrapper
               function so that little of this incompatibilities need be exposed.

  Title:       CONFIGURATIONS WITH TINY MTUS
  Description: Many configurations have the MTU (CONFIG_NET_BUFSIZE) set to very small
               numbers, less then the minimum MTU size that must be supported -- 576.
               This can cause problems in some networks:  CONFIG_NET_BUFSIZE should
               be set to at least 576 in all defconfig files.

               The symptoms of using very small MTU sizes can be very strange.  With
               Ubuntu 9.x and vsFtpd was that the total packet size did *not match* the
               packet size in the IP header.  This then caused a TCP checksum failure
               and the packet was rejected.
  Status:      Open
  Priority:    Low... fix defconfig files as necessary.

o USB (drivers/usbdev, drivers/usbhost)
  ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

  Title:       USB STORAGE DRIVER DELAYS
  Description: There is a workaround for a bug in drivers/usbdev/usbdev_storage.c.
               that involves delays.  This needs to be redesigned to eliminate these
               delays.  See logic conditioned on CONFIG_USBMSC_RACEWAR.
  Status:      Open
  Priority:    Medium

  Title:       RTL8187 DRIVER IS UNFINISHED
  Description: misc/drivers/usbhost_rtl8187.c is a work in progress.  There is no RTL8187
               driver available yet.  That is a work in progress it was abandoned because
               it depends on having an 802.11g stack.
  Status:      Open
  Priority:    Low (Unless you need RTL8187 support).

  Title:       EP0 OUT CLASS DATA
  Description: There is no mechanism in place to handle EP0 OUT data transfers.
               There are two aspects to this problem, neither are easy to fix
               (only because of the number of drivers that would be impacted):

               1. The class drivers only send EP0 write requests and these are
                  only queued on EP0 IN by this drivers.  There is never a read
                  request queued on EP0 OUT.
               2. But EP0 OUT data could be buffered in a buffer in the driver
                  data structure.  However, there is no method currently
                  defined in the USB device interface to obtain the EP0 data.

               Updates:  (1) The USB device-to-class interface as been extended so
               that EP0 OUT data can accompany the SETUP request sent to the
               class drivers. (2) The logic in the STM32 F4 OTG FS device driver
               has been extended to provide this data.  Updates are still needed
               to other drivers.
  Status:      Open
  Priority:    High for class drivers that need EP0 data.  For example, the
               CDC/ACM serial driver might need the line coding data (that
               data is not used currenly, but it might be).

  Title:       USB HUB SUPPORT
  Description: Add support for USB hubs
  Status:      Open
  Priority:    Low/Unknown.  This is a feature enhancement.

o Libraries (libc/)
  ^^^^^^^^^^^^^^^^^

  Title:       SIGNED time_t
  Description: The NuttX time_t is type uint32_t. I think this is consistent
               with all standards and with normal usage of time_t.  However,
               according to Wikipedia, time_t is usually implemented as a
               signed 32-bit value.
  Status:      Open
  Priority:    Very low unless there is some compelling issue that I do not
               know about.

  Title:       ENVIRON
  Description: The definition of environ in stdlib.h is bogus and will not
               work as it should.  This is because the underlying
               representation of the environment is not an arry of pointers.
  Status:      Open
  Priority:    Medium

  Title:       TERMIOS
  Description: Need some minimal termios support... at a minimum, enough to
               switch between raw and "normal" modes to support behavior like
               that needed for readline().
               UPDATE:  There is growing functionality in libc/termios/ and in the
               ioctl methods of several MCU serial drivers (stm32, lpc43, lpc17,
               pic32).  However, as phrased, this bug cannot yet be closed since
               this "growing functionality" does not address all termios.h
               functionality and not all serial drivers support termios.
  Status:      Open
  Priority:    Low

  Title:       DAYS OF THE WEEK
  Description: strftime() and other timing functions do not handle days of the week.
  Status:      Open
  Priority:    Low

  Title:       RESETTING GETOPT()
  Description: There is an issue with the way that getopt() handles errors that
               return '?'.
               
               1. Does getopt() reset its global variables after returning '?' so
                  that it can be re-used?  That would be required to support where
                  the caller terminates parsing before reaching the last parameter.
               2. Or is the client expected to continue parsing after getopt()
                  returns '?'  and parse until the final parameter?
            
               The current getopt() implementation only supports #2.
  Status:      Open
  Priority:    Low

  Title:       FERROR() AND CLEARERR()
  Description: Not implemented: ferror() and clearerr()
  Status:      Open
  Priority:    Low

  Title:       CONCURRENT STREAM READ/WRITE
  Description: NuttX only supports a single file pointer so reads and writes 
               must be from the same position.  This prohibits implementation
               of behavior like that required for fopen() with the "a+" mode.
               According to the fopen man page:
               
               "a+ Open for reading and appending (writing at end of file).
                The file is created if it does not exist. The initial file
                position for reading is at the beginning of the file, but
                output is always appended to the end of the file."

               At present, the single NuttX file pointer is positioned to the
               end of the file for both reading and writing.
  Status:      Open
  Priority:    Medium.  This kind of operation is probably not very common in
               deeply embedded systems but is required by standards.

  Title:       DIVIDE BY ZERO
  Description: This is bug 3468949 on the SourceForge website (submitted by
               Philipp Klaus Krause):
               "lib_strtod.c does contain divisions by zero in lines 70 and 96.
                AFAIK, unlike for Java, division by zero is not a reliable way to
                get infinity in C. AFAIK compilers are allowed e.g. give a compile-
                time error, and some, such as sdcc, do. AFAIK, C implementations
                are not even required to support infinity. In C99 the macro isinf()
                could replace the first use of division by zero. Unfortunately, the
                macro INFINITY from math.h probably can't replce the second division
                by zero, since it will result in a compile-time diagnostic, if the
                implementation does not support infinity."
  Status:       Open
  Priority:     

  Title:       OLD dtoa NEEDS TO BE UPDATED
  Description: This implementation of dtoa in libc/stdio is old and will not
               work with some newer compilers.  See 
               http://patrakov.blogspot.com/2009/03/dont-use-old-dtoac.html
  Status:      Open
  Priority:    ??

  Title:       FLOATING POINT FORMATS
  Description: Only the %f floating point format is supported.  Others are accepted
               but treated like %f.
  Status:      Open
  Priority:    Medium (this might important to someone).

  Title:       FLOATING POINT PRECISION
  Description: A fieldwidth and precision is required with the %f format.  If %f
               is used with no format, than floating numbers will be printed with
               a precision of 0 (effectively presented as integers).
  Status:      Open
  Priority:    Medium (this might important to someone).

o File system / Generic drivers (fs/, drivers/)
  ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

  NOTE:  The NXFFS file system has its own TODO list at nuttx/fs/nxffs/README.txt

  Title:       CHMOD() AND TRUNCATE()
  Description: Implement chmod(), truncate().
  Status:      Open
  Priority:    Low

  Title:       CAN POLL SUPPORT
  Description: At present, the CAN driver does not support the poll() method.
               See drivers/can.c
  Status:      Open
  Priority:    Low

  Title:       REMOVING PIPES AND FIFOS
  Description: There is no way to remove a FIFO or PIPE created in the
               pseudo filesystem.  Once created, they persist indefinitely
               and cannot be unlinked.  This is actually a more generic
               issue:  unlink does not work for anything in the pseudo-
               filesystem.
  Status:      Open, but partially resolved: pipe buffer is at least freed
               when there are not open references to the pipe/FIFO.
  Priority:    Medium

  Title:       ROMFS CHECKSUMS
  Description: The ROMFS file system does not verify checksums on either
               volume header on on the individual files.
  Status:      Open
  Priority:    Low.  I have mixed feelings about if NuttX should pay a
               performance penalty for better data integrity.

  Title:       SPI-BASED SD MULTIPLE BLOCK TRANSFERS
  Description: The simple SPI based MMCS/SD driver in fs/mmcsd does not
               yet handle multiple block transfers.
  Status:      Open
  Priority:    Medium-Low

  Title:       READ-AHEAD/WRITE BUFFER UNTESTED
  Description: Block driver read-ahead buffer and write buffer support is
               implemented but not yet tested.
  Status:      Open
  Priority:    Low

  Title:       SDIO-BASED SD READ-AHEAD/WRITE BUFFERING INCOMPLETE
  Description: The drivers/mmcsd/mmcsd_sdio.c driver has hooks in place to
               support read-ahead buffering and write buffering, but the logic
               is incomplete and untested.
  Status:      Open
  Priority:    Low

  Title:       POLLHUP SUPPORT
  Description: All drivers that support the poll method should also report
               POLLHUP event when the driver is closedd.
  Status:      Open
  Priority:    Medium-Low

  Title:       CONFIG_RAMLOG_CONSOLE DOES NOT WORK
  Description: When I enable CONFIG_RAMLOG_CONSOLE, the system does not come up
               propertly (using configuration stm3240g-eval/nsh2).  The problem
               may be an assertion that is occuring before we have a console.
  Status:      Open
  Priority:    Medium

o Graphics subystem (graphics/)
  ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

  See also the NxWidgets TODO list file for related issues.

  Title:       UNTESTED GRAPHICS APIS
  Description: Testing of all APIs is not complete.  See
               http://nuttx.sourceforge.net/NXGraphicsSubsystem.html#testcoverage
  Status:      Open
  Priority:    Medium

  Title:       ITALIC FONTS / NEGATIVE FONT OFFSETS
  Description: Font metric structure (in include/nuttx/nx/nxfont.h) should allow
               negative X offsets. Negative x-offsets are necessary for certain
               glyphs (and is very common in italic fonts).
               For example Eth, icircumflex, idieresis, and oslash should have
               offset=1 in the 40x49b font (these missing negative offsets are
               NOTE'ed in the font header files).
  Status:      Open.  The problem is that the x-offset is an unsigned bitfield
               in the current structure.
  Priority:    Low.

  Title:       RAW WINDOW AUTORAISE
  Description: Auto-raise only applies to NXTK windows. Shouldn't it also apply
               to raw windows as well?
  Status:      Open
  Priority:    Low

  Title:       AUTO-RAISE DISABLED
  Description: Auto-raise is currently disabled in NX multi-server mode.  The
               reason is complex:
               - Most touchscreen controls send touch data a high rates
               - In multi-server mode, touch events get queued in a message
                  queue.
               - The logic that receives the messages performs the auto-raise.
                 But it can do stupid things after the first auto-raise as
                 it opperates on the stale data in the message queue.
               I am thinking that auto-raise ought to be removed from NuttX
               and moved out into a graphics layer (like NxWM) that knows
               more about the appropriate context to do the autoraise.
  Status:      Open
  Priority:    Medium low

  Title:       IMPROVED NXCONSOLE FONT CACHING
  Description: Now each NxConsole instance has its own private font cache
               whose size is determined by CONFIG_NXCONSOLE_MXCHARS.  If there
               are multiple NxConsole instances using the same font, each will
               have a separate font cache.  This is inefficient and wasteful
               of memory:  Each NxConsole instance should share a common font
               cache.
  Status:      Open
  Priority:    Medium.  Not important for day-to-day testing but would be
               a critical improvement if NxConsole were to be used in a
               product.
 
o Pascal Add-On (pcode/)
  ^^^^^^^^^^^^^^^^^^^^^^

  Title:       P-CODES IN MEMORY UNTESTED
  Description: Need APIs to verify execution of P-Code from memory buffer.
  Status:      Open
  Priority:    Low

  Title:       SMALLER LOADER AND OBJECT FORMAT
  Description: Loader and object format may be too large for some small
               memory systems.  Consider ways to reduce memory footprint.
  Status:      Open
  Priority:    Medium

o Documentation (Documentation/)
  ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

  Title:       DOCUMENT APIS USABLE FROM INTERRUPT HANDLERS
  Description: Need to document which APIs can be used in interrupt
               handlers (like mq_send and sem_post) and which cannot.
  Status:      Open
  Priority:    Low

o Build system
  ^^^^^^^^^^^^

  Title:       NUTTX CONFIGURATION TOOL
  Description: Need a NuttX configuration tool.  The number of configuration
               settings has become quite large and difficult to manage manually.
               Update:  This task is essentially completed.  But probably not for
               all platforms and all features.  When do we know that the feature
               is complete and that we can switch to exclusive use of the tool?
  Status:      Open
  Priority:    Medium-low

  Title:       NATIVE WINDOWS BUILD
  Description: This effort is underway using MinGW-GCC and GNUWin32 tools
               for (coreutils+make+grep+sed+uname).  Current status:

               1. configs/stm32f4discovery/winbuild - builds okay natively
               2. configs/ez80f910200kitg - Can be reconfigured to build natively.
                  Requires some manual intervention to get a clean build.
                  See configs/ez80f910200kitg/README.txt.

  Status:      Open
  Priority:    Low

  Title:       WINDOWS DEPENDENCY GENERATION
  Description: Dependency generation is currently disabled when a Windows native
               toolchain is used in a POSIX-like enviornment (like Cygwin).  The
               issue is that the Windows tool generates dependencies use Windows
               path formatting and this fails with the dependency file (Make.dep)
               is include).  Perhaps the only issue is that all of the Windows
               dependencies needed to be quoted in the Make.dep files.
  Status:      Open
  Priority:    Low -- unless some dependency-related build issues is discovered.

  Title:       SETENV.H
  Description: Logic in most setenv.sh files can create the following problem
               on many platforms:

                 $ . ./setenv.sh
                 basename: invalid option -- 'b'
                 Try `basename --help' for more information.

               The problem is that $0 is the current running shell which may include
               a dash in front:

                 $ echo $0
                 -bash

               But often is just /bin/bash (and the problem does not occur.  The fix
               is:

                 -if [ "$(basename $0)" = "setenv.sh" ]; then
                 +if [ "$_" = "$0" ] ; then
  Status:      Open
  Priority:    Low.  Use of setenv.sh is optional and most platforms do not have
               this problem.  Scripts will be fixed one-at-a-time as is appropropriate.

  Title:       MAKE EXPORT LIMITATIONS
  Description: The top-level Makefile 'export' target that will bundle up all of the
               NuttX libraries, header files, and the startup object into an export-able
               tarball. This target uses the tools/mkexport.sh script.  Issues:

               1. This script assumes the host archiver ar may not be appropriate for
                  non-GCC toolchains
               2. For the kernel build, the user libraries should be built into some
                  libuser.a.  The list of user libraries would have to accepted with
                  some new argument, perhaps -u.
  Status:      Open
  Priority:    Low.

  Title:       KERNEL BUILD MODE ISSUES - GRAPHICS/NSH PARTITIONING.
  Description: In the kernel build mode (where NuttX is built as a monlithic
               kernel and user code must trap into the protected kernel via
               syscalls), the single user mode cannot be supported.  In this
               built configuration, only the multiple user mode can be supported
               with the NX server residing inside of the kernel space.  In
               this case, most of the user end functions in graphics/nxmu
               must be moved to libc/nx and those functions must be built into
               libuser.a to be linked with the user-space code.
               A similar issue exists in NSH that uses some internal OS
               interfaces that would not be available in a kernel build
               (such as foreach_task, foreach_mountpoint, etc.).
  Status:      Open
  Priority:    Low -- the kernel build configuration is not fully fielded
               yet.

  Title:       kconfig-mconf NOT AVAILABLE IN NATIVE WINDOWS BUILD
  Description: NuttX is migrating to the use of the kconfig-frontends kconfig-mconf
               tool for all configurations.  In NuttX 6.24, support for native
               Windows builds was added.  However, thekconfig- mconf tool does not
               build to run natively under Windows.

               Some effort was spent trying to get a clean kconfig-mconf build under
               Windows.  This is documented in the message thread beginning
               here: http://tech.groups.yahoo.com/group/nuttx/message/2900.
               The build was successfully completed using:  MinGW-GCC, MSYS,
               additional Windows libraries, and additional MSYS libraries
               (MSYS is a variant of Cygwin so, presumeably, Cygwin could
               have been used as well).  However, on final testing, it was
               found that there are problems with text and numeric entry:
               http://tech.groups.yahoo.com/group/nuttx/message/2953.  This
               was considered a show stopper and the changs were not checked
               in.

               Options:  (1) Use kconfigs-conf (not kconfig-mconf).  confis the text-only
               configuration tool, (2) fix kconfig-mconf, (3) write another variant
               of the configuration tool for windows, or (4) do all configuration
               under Cygwin or MSYS.  I am doing (4) now, but this is very
               awkward because I have to set the apps path to ../apps (vs
               ..\apps) and CONFIG_WINDOWS_NATIVE=n for the 'make menuconfig'
               to run error free under windows.  Very awkward!
  Status:      Open, there are some workarounds, but none are good.
  Priority:    High

o Linux/Cywgin simulation (arch/sim)
  ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

  Title:       SIMULATED SERIAL DRIVER
  Description: The simulated serial driver has some odd behavior.  It
               will stall for a long time on reads when the C stdio buffers are
               being refilled. This only effects the behavior of things like
               fgetc().  Workaround: Set CONFIG_STDIO_BUFFER_SIZE=0, suppressing
               all C buffered I/O.
  Status:      Open
  Priority:    Low (because the simulator is only a test/development platform)

  Title:       SIMULATOR NETWORKING SUPPORT
  Description: I never did get networking to work on the sim Linux target.  On Linux,
               it tries to use the tap device (/dev/net/tun) to emulate an Ethernet
               NIC, but I never got it correctly integrated with the NuttX networking.
               NOTE: On Cygwin, the build uses the Cygwin WPCAP library and is, at
               least, partially functional (it has never been rigorously tested).
  Status:      Open
  Priority:    Low (unless you want to test networking features on the simulation).
  
  Title:       ROUND-ROBIN SCHEDULING IN THE SIMULATOR
  Description: Since the simulation is not pre-emptible, you can't use round-robin
               scheduling (no time slicing).  Currently, the timer interrupts are
               "faked" during IDLE loop processing and, as a result, there is no
               task pre-emption because there are no asynchrous events.  This could
               probably be fixed if the "timer interrupt" were driver by Linux
               signals. NOTE:  You would also have to implement irqsave() and
               irqrestore() to block and (conditionally) unblock the signal.
  Status:      Open
  Priority:    Low
  
  Title:       NSH ISSUES ON THE SIMULATOR
  Descripion:  The NSH example has some odd behaviors.  Mult-tasking -- for example,
               execution of commands in background -- does not work normally.  This
               is due to the fact that NSH uses the system standard input for the
               console.  This means that the simulation is actually "frozen" all of
               the time when NSH is waiting for input and background commands never
               get the chance to run.
  Status:      Open
  Priority:    This will not be fixed.  This is the normal behavior in the current
               design of the simulator.  "Real" platforms will behave correctly
               because NSH will "sleep" when it waits for console inpu and other
               tasks can run freely.

  Title:       DOUBLE COMMAND ECHO
  Description: In the NSH example, the host HOST echoes each command so after you
               you enter a command, the command is repeated on the next line.  This
               is an artifact of the simulator only.
  Status:      Open
  Priority:    This will not be fixed.  This is the normal behavior in the current
               design of the simulator.  "Real" platforms will behave correctly.

o ARM (arch/arm/)
  ^^^^^^^^^^^^^^^

  Title:       IMPROVED ARM INTERRUPT HANDLING
  Description: ARM interrupt handling performance could be improved in some
               ways. One easy way is to use a pointer to the context save
               area in current_regs instead of using up_copystate so much.
               see handling of 'current_regs" in arch/arm/src/armv7-m/* for
               examples of how this might be done.
  Status:      Open
  Priority:    Low

  Title:       IMPROVED ARM INTERRUPT HANDLING
  Description: The ARM and Cortex-M3 interrupt handlers restores all regisers
               upon return. This could be improved as well:  If there is no
               context switch, then the static registers need not be restored
               because they will not be modified by the called C code.
               (see arch/sh/src/sh1/sh1_vector.S for example)
  Status:      Open
  Priority:    Low

  Title:       ARM INTERRUPTS AND USER MODE
  Description: The ARM interrupt handling (arch/arm/src/arm/up_vectors.S) returns
               using 'ldmia   sp, {r0-r15}^'  My understanding is that this works
               fine because everything is in kernel-mode.  In an operating model
               where applications run in user mode and interrupts/traps run in
               kernel-mode, I think that there is a problem with this.  This would
               like be a problem, for example, if for a kernel build where NuttX
               is built as a monolithic, protected kernel and user mode programs
               trap into the kernel.
  Status:      Open
  Priority:    Low until I get around to implementng security or kernel mode for
               the ARM platform.

  Title:       CORTEX-M3 STACK OVERFLOW
  Description: There is bit bit logic inf up_fullcontextrestore() that executes on
               return from interrupts (and other context switches) that looks like:

                 ldr r1, [r0, #(4*REG_CPSR)] /* Fetch the stored CPSR value */
                 msr cpsr, r1 /* Set the CPSR */

                 /* Now recover r0 and r1 */

                 ldr r0, [sp]
                 ldr r1, [sp, #4]
                 add sp, sp, #(2*4)

                 /* Then return to the address at the stop of the stack,
                  * destroying the stack frame
                  */

                 ldr pc, [sp], #4

               Under conditions of excessivley high interrupt conditions, many
               nested interrupts can oocur just after the 'msr cpsr' instruction.
               At that time, there are 4 bytes on the stack and, with each
               interrupt, the stack pointer may increment and possibly overflow.

               This can happen only under conditions of continuous interrupts.
               See this email thread: http://tech.groups.yahoo.com/group/nuttx/message/1261
               On suggested change is:

                 ldr  r1, [r0, #(4*REG_CPSR)] /* Fetch the stored CPSR value */
                 msr spsr_cxsf, r1 /* Set the CPSR */
                 ldmia     r0, {r0-r15}^

               But this has not been proven to be a solution.
  Status:      Open
  Priority:    Low.  The conditions of continous interrupts is really the problem.
               If your design needs continous interrupts like this, please try
               the above change and, please, submit a patch with the working fix.

  Title:       KERNEL MODE ISSUES - HANDLERS
  Description: The is a design flaw in the ARM/Cortex trap handlers.  Currently,
               they try to process the SYSCALL within the trap handler.  That
               cannot work.  There are two possibilities to fix this.
               1) Just enable interrupts in the trap handler and make sure that
                  that sufficient protection is in place to handler the nested
                  interrupts, or
               3) Return from the exception via a trampoline (such as is
                  currently done for signal handlers).  In the trampoline,
                  the trap would processed in supervisor mode with interrupts
                  enabled.
  Status:      Open
  Priority:    medium-high.

o ARM/C5471 (arch/arm/src/c5471/)
  ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

  Title:       UART RECONFIGURATION
  Description: UART re-configuration is untested and conditionally compiled out.
  Status:      Open
  Priority:    Medium.  ttyS1 is not configured, but not used; ttyS0 is configured
               by the bootloader

o ARM/DM320 (arch/arm/src/dm320/)
  ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

  Title:       DEBUG ISSUES
  Description: config/ntos-dm320: It seems that when a lot of debug statements
               are added, the system no longer boots.  This is suspected to be
               a stack problem: Making the stack bigger or removing arrays on
               the stack seems to fix the problem (might also be the
               bootloader overwriting memory)
  Status:      Open
  Priority:    Medium

  Title:       USB DEVICE DRIVER UNTESTED
  Description: A USB device controller driver was added but has never been tested.
  Status:      Open
  Priority:    Medium

  Title:       FRAMEBUFFER DRIVER UNTESTED
  Description: A framebuffer "driver" was added, however, it remains untested.
  Status:      Open
  Priority:    Medium

  Title:       VIDEO ENCODER DRIVER
  Description: In order to use the framebuffer "driver" additional video encoder
               logic is required to setupt composite video output or to interface
               with an LCD.
  Status:      Open
  Priority:    Medium (high if you need to use the framebuffer driver)

o ARM/i.MX (arch/arm/src/imx/)
  ^^^^^^^^^^^^^^^^^^^^^^^^^^^^

  Title:       PORT IS INCOMPLETE
  Description: The basic port of the i.MX1 architecuture was never finished.  The port
               is incomplete (as of this writing, is still lacks a timer, interrupt
               decoding, USB, network) and untested.
  Status:      Open
  Priority:    Medium (high if you need i.MX1/L support)

  Title:       SPI METHODS ARE NOT THREAD SAFE
  Description: SPI methods are not thread safe.  Needs a semaphore to protect from re-entrancy.
  Status:      Open
  Priority:    Medium -- Will be very high if you do SPI access from multiple threads.

o ARM/LPC17xx (arch/arm/src/lpc17xx/)
  ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

  Title:       USB DMA INCOMPLETE
  Description: USB DMA not fully implemented. Partial logic is in place but it is
               fragmentary and bogus. (Leveraged from the lpc214x)
  Status:      Open
  Priority:    Low

  Title:       SSP DRIVER IMPROVEMENTS
  Description: a) At present the SSP driver is polled.  Should it be interrupt driven?
                  Look at arch/arm/src/imx/imx_spi.c -- that is a good example of an
                  interrupt driven SPI driver.  Should be very easy to part that architecture
                  to the LPC.
               b) See other SSP (SPI) driver issues listed under ARM/LPC214x.  The LPC17xx
                  driver is a port of the LPC214x driver and probably has the same issues.
               b) Other SSP driver improvements: Add support for multiple devices on the
                  SSP bus, use DMA data transfers
  Status:      Open
  Priority:    Medium

  Title:       NOKIA LCD DRIVER NONFUNCTIONAL
  Description: An LCD driver for the Olimex LPC1766STK has been developed.  However, that
               driver is not yet functional on the board:  The backlight comes on, but
               nothing is visible on the display.
  Status:      Open
  Priority:    Medium-Low (unless you need the display on the LPC1766STK!)

o ARM/LPC214x (arch/arm/src/lpc214x/)
  ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

  Title:       VECTOR INTERRUPTS
  Description: Should use Vector Interrupts
  Status:      Open
  Priority:    Low

  Title:       USB DMA INCOMPLETE
  Description: USB DMA not fully implemented. Partial logic is in place but it is
               fragmentary and bogus.
  Status:      Open
  Priority:    Low

  Title:       USB SERIAL DRIVER REPORTS WRONG ERROR
  Description: USB Serial Driver reports wrong error when opened before the
               USB is connected (reports EBADF instead of ENOTCONN)
  Status:      Open
  Priority:    Low

  Title:       SPI DRIVER IMPROVEMENTS
  Description: At present the SPI driver is polled.  Should it be interrupt driven?
               Look at arch/arm/src/imx/imx_spi.c -- that is a good example of an
               interrupt driven SPI driver.  Should be very easy to part that architecture
               to the LPC.
  Status:      Open
  Priority:    Medium

  Title:       SPI METHODS ARE NOT THREAD SAFE
  Description: SPI methods are not thread safe.  Needs a semaphore to protect from re-entrancy.
  Status:      Open
  Priority:    Medium -- Will be very high if you do SPI access from multiple threads.

  Title:       SPI DRIVER DELAYS
  Description: At present the SPI driver is polled -AND- there is a rather large, arbitrary,
               delay in one of the block access routines.  The purpose of the delay is to
               avoid a race conditions.  This begs for a re-design -OR- at a minimum, some
               optimiation of the delay time.
  Status:      Open
  Priority:    Medium

  Title:       2GB SD CARD ISSUES
  Desription:  I am unable to initialize a 2Gb SanDisk microSD card (in adaptor) on the
               the mcu123 board.  The card fails to accept CMD0.  Doesn't seem like a software
               issue, but if anyone else sees the problem, I'd like to know.
               Related:  Fixes were recently made for the SDIO-based MMC/SD driver to
               support 2Gb cards -- the blocksize was forced to 512 in all cases.  The SPI-
               based driver may also have this problem (but I don't think this would have
               anything to do with CMD0).
  Status:      Open
  Priority:    Uncertain

  Title:       USB BROKEN?
  Description: I tried to bring up the new configuration at configs/mcu123-214x/composite,
               and Linux failed to enumerate the device.  I don't know if this is 
               a problem with the lpc214x USB driver (bit rot), or due to recent
               changed (e.g., -r4359 is suspicious), or an incompatibility between the
               Composite driver and the LPC214x USB driver.  It will take more work
               to find out which -- like checking if the other USB configurations are
               also broken.
  Status:      Open
  Priority:    It would be high if the LPC2148 were a current, main stream architecture.
               I am not aware of anyone using LPC2148 now so I think the priority has
               to be low.

o ARM/LPC31xx (arch/arm/src/lpc31xx/)
  ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

  Title:       PLATFORM-SPECIFIC LOGIC
  Description: arch/arm/src/lpc313x/lpc313x_spi.c contains logic that is specific to the
               Embedded Artist's ea3131 board.  We need to abstract the assignment of SPI
               chip selects and logic SPI functions (like SPIDEV_FLASH).  My thoughts are:
               - Remove lpc313x_spiselect and lpc313x_spistatus from lpc313x_internal.h
               - Remove configs/ea3131/src/up_spi.c
               - Add configurations CONFIG_LPC3131x_CSOUT1DEV, CONFIG_LPC3131x_CSOUT2DEV,
                 and CONFIG_LPC3131x_CSOUT3DEV that maps the lpc313x SPI chip selects to
                 SPIDEV_* values.
               - Change arch/arm/src/lpc313x/lpc313x_spi.c to use those configuration
                 settings.
  Status:      Open
  Priority:    High if you want to use SPI on any board other than the ea3131.

  Title:       SPI DRIVER
  Description: arch/arm/src/lpc313x/lpc313x_spi.c may or may not be functional.  It was
               reported to be working, but I was unable to get it working with the
               Atmel at45dbxx serial FLASH driver.
  Status:      Open
  Priority:    High if you need to use SPI.

o ARM/LPC43x (arch/arm/src/lpc43xx/)
  ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

o ARM/STR71x (arch/arm/src/str71x/)
  ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

  Title:       UNVERIFIED MMC SUPPORT
  Description: Verify SPI driver and integrate with MMC support. This effort is stalled
               at the moment because the slot on the Olimex board only accepts MMC card;
               I have no MMC cards, only SD cards which won't fit into the slot.
  Status:      Open
  Priority:    Medium

  Title:       NO USB DRIVER
  Description: Develop a USB driver and integrate with existing USB serial and storage
               class drivers.
  Status:      Open
  Priority:    Medium

  Title:       SPI METHODS ARE NOT THREAD SAFE
  Description: SPI methods are not thread safe.  Needs a semaphore to protect from re-entrancy.
  Status:      Open
  Priority:    Medium -- Will be very high if you do SPI access from multiple threads.

o ARM/LM3S6918 (arch/arm/src/lm/)
  ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

  Title:       I2C DRIVER
  Description: Still need to implement I2C
  Status:      Open
  Priority:    Low

  Title:       SSI OVERRUNS
  Description: Should terminate SSI/SPI transfer if an Rx FIFO overrun occurs.
               Right now, if an Rx FIFO overrun occurs, the SSI driver hangs.
  Status:      Open
  Priority:    Medium, If the transfer is properly tuned, then there should not
               be any Rx FIFO overruns.

  Title:       THTTPD BUGS
  Description: There are some lingering bugs in THTTPD, possibly race conditions.  This
               is covered above under Network Utilities, but is duplicated here
               to point out that the LM3S suffers from this bug.
  Status:      Open.
               UPDATE: I have found that increasing the size of the CGI program stack
               from 1024 to 2048 (on the LM3S) eliminates the problem.  So the most
               likely cause is probably a stack overflow, not a hard sofware bug.
  Priority:    Probably Low

o ARM/STM32 (arch/arm/src/stm32/)
  ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

  Title:       USBSERIAL ISSUES
  Description  A USB device-side driver is in place but not well tested.  At
               present, the apps/examples/usbserial test sometimes fails.  The situation
               that causes the failure is:

               - Host-side of the test started after the target side sends the
                 first serial message.

               The general failure is as follows:

               - The target message pends in the endpoint packet memory
               - When the host-side of the test is stated, it correctly
                 reads this pending data.
               - an EP correct transfer interrupt occurs and the next
                 pending outgoing message is setup
               - But, the host never receives the next message

               If the host-side driver is started before the first target message
               is sent, the driver works fine.
  Status:      Open
  Priority:    Medium-High
  
  Title:       DMA EXTENSIONS
  Description: DMA logic needs to be extended.  DMA2, Channel 5, will not work
               because the DMA2 channels 4 & 5 share the same interrupt.
  Status:      Open
  Priority:    Low until someone needs DMA1, Channel 5 (ADC3, UART4_TX, TIM5_CH1, or
               TIM8_CH2).

  Title:       F4 SDIO MULTI-BLOCK TRANSFER FAILURES
  Description: If you use a large I/O buffer to access the file system, then the
               MMCSD driver will perform multiple block SD transfers.  With DMA
               ON, this seems to result in CRC errors detected by the hardware
               during the transfer.  Workaround:  CONFIG_MMCSD_MULTIBLOCK_DISABLE=y.
  Status:      Open
  Priority:    Medium

  Title:       DMA BOUNDARY CROSSING
  Description: I see this statement in the reference manual:  "The burst
               configuration has to be selected in order to respect the AHB protocol,
               where bursts must not cross the 1 KB address boundary because the
               minimum address space that can be allocated to a single slave
               is 1 KB. This means that the 1 KB address boundary should not be crossed
               by a burst block transfer, otherwise an AHB error would be generated,
               that is not reported by the DMA registers."

               The implication is that there may be some unenforced alignment
               requirements for some DMAs.  There is nothing in the DMA driver to
               prevent this now.
  Status:      Open
  Priority:    Low (I am not even sure if this is a problem yet).

  Title:       DMA FROM EXTERNAL, FSMC MEMORY
  Description: I have seen a problem on F1 where all SDIO DMAs work exist for
               write DMAs from FSMC memory (i.e., from FSMC memory to SDIO).
               Read transfers work fine (SDIO to FSMC memory).  The failure is
               a data underrun error with zero bytes of data transferred.  The
               workaround for now is to use DMA buffers allocted from internal
               SRAM.
  Status:      Open
  Priority:    Low

o AVR (arch/avr)
  ^^^^^^^^^^^^^^

  Title:        AMBER WEB SERVER UNTESTED
  Description:  There is a port for the Amber Web Server ATMega128, however this is
                completely untested due to the lack to compatible, functional test
                equipment.
  Status:       Open
  Priority:     The priority might as well be low since there is nothing I can do about
                it anyway.

  Title:        STRINGS IN RAM
  Description:  Many printf-intensive examples (such as the OS test) cannot be executed
                on most AVR platforms.  The reason is because these tests/examples
                generate a lot of string data.  The build system currently places all
                string data in RAM and the string data can easily overflow the tiny
                SRAMs on these parts.  A solution would be to put the string data
                into the more abundant FLASH memory, but this would require modification
                to the printf logic to access the strings from program memory.
  Status:       Open
  Priority:     Low.  The AVR is probably not the architecuture that you want to use
                for extensive string operations.

  Title:        SPI AND USB DRIVERS UNTESTED
  Description:  An SPI driver and a USB device driver exist for the AT90USB (as well
                as a USB mass storage example).  However, this configuration is not
                fully debugged as of the NuttX-6.5 release.
                Update 7/11:  (1) The SPI/SD driver has been verified, however, (2) I
                believe that the current teensy/usbstorage configuration uses too
                much SRAM for the system to behave sanely.  A lower memory footprint
                version of the mass storage driver will be required before this can
                be debugged
  Status:       Open
  Priority:     Medium-High.

  Title:        AVR32 PORT IS NOT FULLY TESTED
  Description:  A complete port for the AVR32 is provided and has been partially
                debugged.  There may still be some issues with the serial port
                driver.
  Status:       Open
  Priority:     Medium

o Intel x86 (arch/x86)
  ^^^^^^^^^^^^^^^^^^^^

o 8051 / MCS51 (arch/8051/)
  ^^^^^^^^^^^^^^^^^^^^^^^^^

  Title:       STACK OVERFLOWS DURING INTERRUPT HANDLING
  Description: Current status:
               - Basic OS task management seems OK
               - Fails when interrupts enabled.  The stack pointer is around
                 0x6e before the failure occurs.  It looks like some issue
                 when the stack pointer moves from the directly to indirectly
                 addressable region (0x80 boundary).
               - Work on the 8052 is temporarily on hold
  Status:      Open
  Priority:    Low, 8051 is a tough platform because of the tiny stack.

  Title:       TIMER 0 AS SYSTEM TIMER
  Description: Use timer 0 as system timer.  Timer 2 is needed for second UART.
               Logic is implemented, but there needs to be a system
               configuration to change the ticks-per-second value to match the
               timer interrupt rate
  Status:      Open
  Priority:    Low

  Title:       OVERFLOWS DURING BUILD
  Description: During build, there are several integer overflows reported:
               sched/gmtime_r.c aroud lines 184 and 185
               sched/clock_initialize.c at line 107
               sched/pthread_create.c at 330
               apps/examples/ostest/barrier.c around lines 53 and 74
               apps/examples/ostest/sighand.c at 225 and 244
               driver/serial.c in usleep calls around 347 and 354
  Status:      Open.  Update:  These were reviewed during the hcs12 port.  The
               hcs12 also has 16-bit integer types (if -mshort is in the CFLAGS).
               I believe that the warnings in most of the above have been fixed
               but this has not been verified on this platform).
  Priority:    Medium

  Title:       DATA INITIALIZATION
  Description  Global data is not being initialized.  Logic like that of SDCCs
               crt0*.s needs to be incorporated into the system boot logic
  Status:      Open
  Priority:    Low -- only because there as so many other issues with 8051

  Title:       8051 BUILD BROKEN
  Description: The last time I tried to build the pjrc-8051 configurtion using
               the SDCC 3.2.1 toolchain (for Windows).  I got compilation
               errors in sched/os_bringup.c.  It complained about type
               mis-matches.  What I gather from Googling, this is a problem
               with the --stack-auto option.  At any rate, this problem will
               need to be fixed if you want to resurrect the 8051 NuttX port.
 Status:       Open
 Priority:     Low -- I don't think anyone uses the 8051 port.

o MIPS/PIC32(arch/mips)
  ^^^^^^^^^^^^^^^^^^^^^

  Title:       PIC32 USB DRIVER DOES NOT WORK WITH MASS STORAGE CLASS
               UPDATE:  ** ONLY USING RAM DISK FOR EXPORTED VOLUME ***
  Description: The PIC32 USB driver either crashes or hangs when used with
               the mass storage class when trying to write files to the target
               storage device.  This usually works with debug on, but does not
               work with debug OFF (implying some race condition?)

               Here are some details of what I see in debugging:

               1. The USB MSC device completes processing of a read request
                  and returns the read request to the driver.
               2. Before the MSC device can even begin the wait for the next
                  driver, many packets come in at interrupt level.  The MSC
                  device goes to sleep (on pthread_cond_wait) with all of the
                  read buffers ready (16 in my test case).
               3. The pthread_cond_wait() does not wake up.  This implies
                  a problem with pthread_con_wait(?).  But in other cases,
                  the MSC device does wake up, but then immediately crashes
                  because its stack is bad.
               4. If I force the pthread_cond_wait to wake up (by using
                  pthread_cond_timedwait instead), then the thread wakes
                  up and crashes with a bad stack.

               So far, I have no clue why this is failing.

               UPDATE:  This bug was recorded using the PIC32 Ethernet
               Starter kit with a RAM disk (that board has no SD card slot).
               Howevever, using the USB mass storage device with the
               Mikroelektronika using a real SD card, there is no such
               problem -- the mass storage device seems quite stable.

               UPDATE:  Hmmm.. retesting with the Mikroelectronka board
               shows problems again.  I think that there are some subtle
               timing bugs whose effects can very from innocuous to severe.
  Status:      Open
  Priority:    Originally, High BUT reduced to very Low based on the
               UPDATED comments.

  Title:       PIC32 USB MASS STORAGE DEVICE FAILS TO RE-CONNECT
  Description: Found using configuration configs/pic32mx7mmb/nsh.
               In this configuratin, the NSH 'msconn' command will connect the
               mass storage device to the host; the 'msdis' command will
               disconnect the device.  The first 'msconn' works perfectly.
               However, when attempting to re-connect, the second 'msconn'
               command does not command properly:  Windows reports an
               unrecognized device.  Apparently, some state is being properly
               reset when the mass storage device is disconnected.  Shouldn't
               be hard to fix.
  Status:      Open
  Priority:    Medium

  Title:       POSSIBLE INTERRUPT CONTROL ISSUE
  Description: There is a kludge in the file arch/mips/src/common/up_idle.c.
               Basically, if there is nothing else going on in the IDLE loop,
               you have to disable then re-enable interrupts.  Logically nothing
               changes, but if you don't do this interrupts will be be disabled
               in the IDLE loop which is a very bad thing to happen.

               Some odd behavior in the interrupt setup on the IDLE loop is
               not really a big concern, but what I do not understand is if
               this behavior is occurring on all threads after all context
               switches:  Are interrupts always disabled until re-enabled?
               This requires some further investigation at some point; it
               may be nothing but may also be a symptom of some changes
               required to the interrupt return logic (perhaps some CP0
               status hazard?)
  Status:      Open
  Priority:    Low. Puzzling and needs some investigation, but there there
               is no known misbehavior.

o Hitachi/Renesas SH-1 (arch/sh/src/sh1)
  ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

  Title:        SH-1 IS UNUSABLE
  Description:  There are instabilities that make the SH-1 port un-usable.  The
                nature of these is not understood; the behavior is that certain SH-1
                instructions stop working as advertised.  I have seen the following
                examples:

                  412b jmp @r1 - Set a return address in PR, i.e., it behaved like
                       410b jsr @r1.  Normally 412b works correctly, but in the failure
                       condition, it reliably set the PR.
                  69F6 mov.l @r15+,r9 - wrote the value of R1 to @r15+.  This behavior
                       does not correspond to any known SH-1 instruction

                This could be a silicon problem, some pipeline issue that is not
                handled properly by the gcc 3.4.5 toolchain (which has very limit
                SH-1 support to begin with), or perhaps with the CMON debugger.  At
                any rate, I have exhausted all of the energy that I am willing to put
                into this cool old processor for the time being.

                Update:  This bug will probably never be addressed now.  I just
                cleaned house and my old SH-1 was one of the things that went.

  Status:       Open
  Priority:     Low -- because the SH-1, SH7032, is very old and only of historical
                interest.

o Renesas M16C/26 (arch/sh/src/m16c)
  ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

  Title:        M16C DOES NOT BUILD
  Description:  The M16C target cannot be built.  The GNU m16c-elf-ld link fails with 
                the following message:

                m32c-elf-ld: BFD (GNU Binutils) 2.19 assertion fail /home/Owner/projects/nuttx/buildroot/toolchain_build_m32c/binutils-2.19/bfd/elf32-m32c.c:482

                Where the reference line is:

                /* If the symbol is out of range for a 16-bit address,
                   we must have allocated a plt entry.  */
                BFD_ASSERT (*plt_offset != (bfd_vma) -1);

                No workaround is known at this time.
  Status:       Open
  Priority:     High -- this is a show stopper for M16C.

  Title:       M16C PORT UNTESTED
  Description: Coding of the initial port is complete, but is untested.
  Status:      Open
  Priority:    Low

  Title:       NO SERIAL CONNECTOR
  Description: Serial drivers were developed for the M16C, however, the SKP16C26
               StarterKit has no serial connectors.
  Status:      Open
  Priority:    Low

  Title:       UNIMPLEMENTED M16C DRIVERS
  Description: Should implement SPI, I2C, Virual EEPROM, FLASH, RTC drivers
  Status:      Open
  Priority:    Medium

o z80/z8/ez80/z180 (arch/z80)
 ^^^^^^^^^^^^^^^^^^^^^^^^^^^^

  Title:       SDCC INTEGER OVERFLOWS
  Description: The SDCC version the same problems with integer overflow during
               compilation as described for pjrc-8051.  At typical cause is code like
               usleep(500*1000) which exceeds the range of a 16-bit integer.
  Status:      See pjrc-8051.  These have probably been fixed but have not yet
               been verified on these platforms.
  Priority:    See pjrc-8051

  Title:       Z80 SIMULATED CONSOLE
  Description: The simulated Z80 serial console (configs/z80sim/src/z80_serial.c +
               driver/serial.c) does not work.  This is because there are
               no interrupts in the simulation so there is never any serial
               traffic.
  Status:      Open
  Priority:    Low -- the simulated console is not critical path and the designs
               to solve the problem are complex.

  Title:       ZDS-II LIBRARIAN WARNINGS
  Description: ZDS-II Librarian complains that the source for the .obj file
               is not in the library.
  Status:      Open
  Priority:    Low, thought to be cosmetic.  I think this is a consequence of
               replacing vs. inserting the library.

  Title:       ZDS-II COMPILER PROBLEMS
  Description: The ZDS-II compiler (version 4.10.1) fails with an internal error
               while compiler mm/mm_initialize.  This has been reported as
               incident 81509.

               I have found the following workaround that I use to build for the
               time being:

               --- mm/mm_initialize.c.SAVE    2008-02-13 08:06:46.833857700 -0600
               +++ mm/mm_initialize.c    2008-02-13 08:07:26.367608900 -0600
               @@ -94,8 +94,11 @@
               {
                  int i;

               +#if 0 /* DO NOT CHECK IN */
                  CHECK_ALLOCNODE_SIZE;
                  CHECK_FREENODE_SIZE;
               +#endif

               /* Set up global variables */

  Status:      Open
  Priority:    High

  Title:       EZ8 PRIORITY INTERRUPTS
  Description: Add support for prioritized ez8 interrupts.  Currently logic supports
               only nominal interrupt priority.
  Status:      Open
  Priority:    Low

  Title:       Z8ENCORE ONLY VERIFIED ON SIMULATOR
  Description: The z8Encore! port has only been verified on the ZDS-II instruction
               set simulator.
  Status:      Open
  Priority:    Medium

  Title:       XTRS CLEAN
  Description: The XTRS target (configs/xtrs) has a clean problem. The clean
               rule removes .asm files.  This works because there are no .asm
               files except in sub-directories that are provided from 'make clean' --
               except for XTRS:  It has a .asm file in its src/ directory that
               gets removed everytime clean is performd.
  Status:      Open
  Priority:    High if you happen to be working with XTRS.

  Title:       SPI/I2C UNTESTED
  Description: A "generic" SPI and I2C drivers have been coded for the eZ80Acclaim!
               However, these remains untested since I have no SPI or I2C devices for
               the board (yet).
  Status:      Open
  Priority:    Med

  Title:       SPI METHODS ARE NOT THREAD SAFE
  Description: SPI methods are not thread safe.  Needs a semaphore to protect from re-entrancy.
  Status:      Open
  Priority:    Medium -- Will be very high if you do SPI access from multiple threads.

  Title:       I2C UNTESTED
  Description: A "generic" I2C driver has been coded for the eZ8Encore!
               However, this remains untested since I have no I2C devices for
               the board (yet).
  Status:      Open
  Priority:    Med

  Title:       UNFINISHED Z180 LOGIC NEEDED BY THE P112 BOARD
  Description: 1) Need to revist the start-up logic.  Looking at the P112 Bios
                  (Bios.mcd), I see that quite of bit of register setup is done
                  there.
               2) Finish ESCC driver logic.
  Status:      Open
  Priority:    Low (at least until I get P112 hardware)

o z16 (arch/z16)
^^^^^^^^^^^^^^^^

  Title:       ZDS-II LIBRARIAN WARNINGS
  Description: ZDS-II Librarian complains that the source for the .obj file
               is not in the library.
  Status:      Open
  Priority:    Low, thought to be cosmetic.  I think this is a consequence of
               replacing vs. inserting the library.

  Title:       SERIAL DRIVER HANGS
  Description: When the interrupt-driven serial driver is used, the system
               hangs.  This is because of TX ready (TRDE) interrupts that
               get lost while interrupts are disabled.  The existing
               serial driver appears to be limited to hardware with a
               latching, level-sensitive TX ready interrupt.
  Status:      Open
  Priority:    Medium. A polled, write-only serial driver is used in the
               interim for system testing.

  Title:       SYSTEM DELAYS
  Description: The system delays do not appear to be correct with the
               apps/examples/ostest/timedmqueue.c test.
  Status:      Open
  Priority:    Medium-High

  Title:       PROBLEMS WHEN DEBUG DISABLED
  Description: At present, the z16f port does not run properly when CONFIG_DEBUG
               is disabled:  The obvious symptom is that there is no printf()
               output.  I have isolated with problem to errors in optimization.
               With -reduceopt on the command line, I can get the printf output.
               However, there are still errors in the compiled code -- specifically
               in sched/timer_create.c.

               I have submitted a bug report to ZiLOG for this (support incident
               81400).  You can see the status of the bug report (and lots more
               technical detail) here:
               http://support.zilog.com/support/incident/incident_support.asp?iIncidentId=81400&iSiteId=1&chLanguageCode=ENG

               Summary of ZiLOG analysis: "This is a ZNEO compiler problem. ... [a] workaround
               is to replace:
                   if ( !timerid || (clockid != 0) )
                By:
                   if ((clockid != 0) || !timerid)"

  Status:      Open
  Priority:    Medium-High

  Title:       PASCAL ADD-ON
  Description: The pascal add-on does not work with the z16f (that is
               configuration z16f2800100zcog/pashello).  This appears to be
               another ZDS-II error:  when executing the instruction
               SYSIO 0, WRITESTR a large case statement is executed.  This
               involves a call into the ZiLOG runtime library to __uwcase().
               __uwcase is passed a pointer to a structure containing jump
               information.  The cause of the failure appears to be that
               the referenced switch data is bad.
               This is submited as ZiLOG support incident 81459.

               Summary of ZiLOG analysis: "This is a ZNEO run time library problem.
               One workaround is to replace the line 58 in uwcase.asm

               From:
                      ADD       R9,#4             ; Skip handler
               To:
                      ADD       R9,#2             ; Skip handler

               And add uwcase.asm to the project.

               If the customer does not want to modify uwcase.asm then the other
               workaround is to add a dummy case and make it same as default:

               case 0x8000:
               default:

               This will make sure that uwcase is not called but ulcase is called."
  Status:      Open.  Due to licensing issues, I cannot include the modified
               uwcase in the NuttX code base.
  Priority:    Medium

  Title:       USE SPOV
  Description: Add support to maintain SPOV in context switching.  This
               improvement will provide protection against stack overflow
               and make a safer system solution.
  Status:      Open
  Priority:    Low

  Title:       PRIORITIZED INTERRUPTS
  Description: Add support for prioritized interrupts.  Currently logic supports
               only nominal interrupt priority.
  Status:      Open
  Priority:    Low

  Title:       ZDS-II COMPILER PROBLEMS
  Description: The file drivers/mmcsd/mmcsd_sdio.c generates an internal compiler
               error like:
 
               mmcsd\mmcsd_sdio.c
               Internal Error(0503) On line 2504 of "MMCSD\MMCSD_SDIO.C"
                   File <c3>, Args(562,46)

  Status:      Open.  Recommended workaround: remove mmcsd_sdio.c from
               drivers/mmcsd/Make.defs.  There is no SDIO support for the Z16 anyway
  Priority:    Low

  Title:       NATIVE BUILD PROBLEMS
  Description: When last tested (ca.12/12), there were some missing .obj files in
               arch/z16/src. A little additional TLC will be needed to get a
               reliable Windows native build.  As of this writing, the Cygwin
               based build has not been re-verified.
  Status:      Open
  Priority:    Low -- I don't think anyone uses the Z16 port.  

o mc68hc1x (arch/hc)
  ^^^^^^^^^^^^^^^^^^

  Title:       BANKED MODE
  Description: There is no script for building in banked mode (more correctly, there
               is a script, but logic inside the script has not yet been implemented).
               It would be necessary to implement banked mode to able to access more
               the 48K of FLASH.
  Status:      Open.
  Priority:    Medium/Low

o Network Utilities (apps/netutils/)

  Title:       UIP RESOLVER
  Description: One critical part of netutils/ apps is untested: The uIP
               resolver in netutils/resolv.  The webclient code has been
               tested on host using gethosbyname(), but still depends on the
               untested resolve logic.
  Status:      Open
  Priority:    Medium, Important but not core NuttX functionality

  Title:       PPP PORT
  Description: Port PPP support from http://contiki.cvs.sourceforge.net/contiki/contiki-2.x/backyard/core/net/ppp/
  Status:      Open
  Priority:    Low

  Title:       UNVERIFIED THTTPD FEATURES
  Description: Not all THTTPD features/options have been verified.  In particular, there is no
               test case of a CGI program receiving POST input.  Only the configuration of
               apps/examples/thttpd has been tested.
  Status:      Open
  Priority:    Medium

  Title:       THE ARP ISSUES AGAIN
  Description: The first GET received by THTTPD is not responded to.  Refreshing the page
               from the browser solves the problem and THTTPD works fine after thatg.  I 
               believe that this is the duplicate of another bug: "Outgoing [uIP] packets are dropped
               and overwritten by ARP packets if the destination IP has not been mapped to a MAC."
  Status:      Open
  Priority:    Medium

  Title:       THTTPD WARNINGS
  Description: If the network is enabled, but THTTPD is not configured, it spews out lots
               of pointless warnings.  This is kind of annoying and unprofessional; needs to
               be fixed someday.
  Status:      Open.  An annoyance, but not a real problem.
  Priority:    Low

o NuttShell (NSH) (apps/nshlib)
  ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

  Title:       WGET UNTESTED
  Description: The wget command has been incorporated into NSH, however
               it is still untested as of this writing (only because I
               have not had the correct network setup for the testing
               yet).  Since wget depends on the also untest uIP resolv/
               logic, it is like non-functional.
  Status:      Open
  Priority:    Med-High

  Title:       IFCONFIG AND MULTIPLE NETWORK INTERFACES
  Descripton:  The ifconfig command will not behave correctly if an interface
               is provided and there are multiple interfaces.  It should only
               show status for the single interface on the command line; it will
               still show status for all interfaces.
  Status:      Open
  Priority:    Low (multiple network interfaces not fully supported yet anyway).

  Title:       RUN NXFLAT PROGRAMS
  Description: Add support to NSH to run NXFLAT programs from a ROMFS file system
  Status:      Open
  Priority:    Low (enhancement)

  Title:       ARP COMMAND
  Description: Add an ARP command so that we can see the contents of the ARP table.
  Status:      Open
  Priority:    Low (enhancement)

  Title:       RE-DIRECTION OF BUILTIN APPLICATONS
  Description: There is a problem with the re-direction of output form built-in
               applications in NSH.  When output is re-directed, exec_builtin()
               spawns a tiny trampoline task that re-directs the output as
               requested, starts the built-in task and then exit.

               The problem is that when exec_builtin() starts the trampoline task,
               it receives and returns the pid of the trampoline task, and *not*
               the pid of the desired builtin application.  This bad pid is returned
               to NSH and when NSH tries to use that pid in the waitpid() call, it
               fails because the trampoline task no longer exists.

               The same tasking arrangement is used by the standard function
               posix_spawn().  However, posix_spawn uses the non-standard, internal
               NuttX interface task_reparent() to replace the childs parent task
               with the caller of posix_spawn().

               exec_builtin() should not use this internal interface, however,
               since it resides in the application space.  The suggested solution
               is (1) move the exec_builtin() logic into nuttx/sched, (2) make it
               a semi-standard interface renamed to task_spawn() and prototyped
               in nuttx/include/sched.h, and then (2) use task_reparent to solve
               the parental problem in the same way that posix_spawn does.
  Status:      Open
  Priority:    Medium

o System libraries apps/system (apps/system)
  ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

  Title:       READLINE IMPLEMENTATION
  Description: readline implementation does not use C-buffered I/O, but rather
               talks to serial driver directly via read().  It includes VT-100
               specific editting commands.  A more generic readline() should be
               implemented using termios' tcsetattr() to put the serial driver
               into a "raw" mode.
  Status:      Open
  Priority:    Low (unless you are using mixed C-buffered I/O with readline and
               fgetc, for example).

o Other Applications & Tests (apps/examples/)
  ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

  Title:       EXAMPLES/PIPE ON CYGWIN
  Description: The redirection test (part of examples/pipe) terminates
               incorrectly on the Cywgin-based simulation platform (but works
               fine on the Linux-based simulation platform).
  Status:      Open
  Priority:    Low

  Title:       EXAMPLES/WGET UNTESTED
  Description: examples/wget is untested on the target (it has been tested
               on the host, but not in the target using the uIP resolv logic).
  Status:      Open
  Priority:    Med

  Title:       EXAMPLES/SENDMAIL UNTESTED
  Description: examples/sendmail is untested on the target (it has been tested
               on the host, but not on the target).
  Status:      Open
  Priority:    Med

  Title:       EXAMPLES/NX FONT CACHING
  Description: The font caching logic in examples/nx is incomplete.  Fonts are
               added to the cache, but never removed.  When the cache is full
               it stops rendering.  This is not a problem for the examples/nx
               code because it uses so few fonts, but if the logic were
               leveraged for more general purposes, it would be a problem.
               Update: see examples/nxtext for some improved font cache handling.
  Status:      Open
  Priority:    Low.  This is not really a problem becauses examples/nx works
               fine with its bogus font caching.

  Title:       EXAMPLES/NXTEXT ARTIFACTS
  Description: examples/nxtext.  Artifacts when the pop-up window is opened.
               There are some artifacts that appear in the upper left hand
               corner.  These seems to be related to window creation.  At
               tiny artifact would not be surprising (the initial window
               should like at (0,0) and be of size (1,1)), but sometimes
               the artifact is larger.
  Status:      Open
  Priority:    Medium.
