#!/bin/sh
#
# @name Generic Hexarotor coaxial geometry
#
# @type Hexarotor Coaxial
# @class Copter
#
# @output MAIN1 front right top, CW; angle:60; direction:CW
# @output MAIN2 front right bottom, CCW; angle:60; direction:CCW
# @output MAIN3 back top, CW; angle:180; direction:CW
# @output MAIN4 back bottom, CCW; angle:180; direction:CCW
# @output MAIN5 front left top, CW; angle:-60; direction:CW
# @output MAIN6 front left bottom, CCW;angle:-60; direction:CCW
#
# @output AUX1 feed-through of RC AUX1 channel
# @output AUX2 feed-through of RC AUX2 channel
# @output AUX3 feed-through of RC AUX3 channel
#
# @maintainer Lorenz Meier <lorenz@px4.io>
#
# @board intel_aerofc-v1 exclude
# @board bitcraze_crazyflie exclude
#

sh /etc/init.d/rc.mc_defaults

set MIXER hexa_cox

# Need to set all 8 channels
set PWM_OUT 12345678
