#!/bin/sh
#
# Board specific specific board MAVLink startup script.
#------------------------------------------------------------------------------

# Start MAVLink on the USB port
mavlink start -d /dev/ttyACM0
